**BID OF : (***Firm Name***)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**PROJECT: 30 /2020-21 – ALTERATION OF GARAGE FOR SUBSTATION AND PUMP HOUSE ATTENDENT LIVING AT ARMY INSTITUTE OF MANAGEMENT NEW CAMPUS AT RAJARHAT, KOLKATA**

*. Please attach supporting drawings, technical literature / brochure, scanned documents / proof etc as applicable.*

*2. Vendors should be prepared to produce product samples, if applicable.*

*3. The bid preferably be typed on letter head of the firm and authenticated by office stamp & signature on each page.*

*4. Rate quoted should be inclusive of transportation, freight, cartage, handling, fabrication / construction, installation, testing and commissioning at the indicated site, warranty / guarantee liability costs, taxes and levies and any special requirements given in the tender document.*

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S No | Brief Description / Specifications of Job / Work / Product) or Item(s) | Accounting Unit | Quantity | Rate | Amount | Remarks |
| 1. | **Provision of Half Brick Masonry Walls** .  Brickwork in CM 1:6.Plaster on both surfaces in CM 1:4.  Two coats of dry distemper. | Sqft | 420 |  |  |  |
| 2. | 2. **Provision of Openings : Doors / Windows / Ventilators** .  (a) 1 x Single Panel Wooden (Pine) Door (6’ x 2.5’) with frame (Sal) and accessories complete ( inside / outside - locking arrangements– tower &/or sliding bolts, handles, stoppers etc).  (b) PVC Door (6’ x 2.5’) with frame and accessories complete ( inside / outside - locking arrangements– tower &/or sliding bolts, handles, stoppers etc).  (c)Aluminium Sliding Window (3’ x 2.5’) with security grill, mosquito proofing and accessories complete (handles etc).  (d) Ventilator (7’ x 2’) in aluminium frame, 3 equal panels – 2 with fixed glazing & 1 with sliding window. With security grill, mosquito proofing and accessories complete (handles etc).  (e) Ventilator (2’ x 1’) in aluminium frame, security grill, mosquito proofing, frosted glass louvere partitions / design. | Nos  Nos  Nos  Nos  Nos | 01  02  01  01  01 |  |  |  |
| 3. | **RCC Work** .  (a) Provision of 9” thick RCC Roof over toiiet with waterproofing treatment.  (b) Provision of RCC Lintel over openings. | Cuft  Cuft | 32  05 |  |  |  |
| 4. | **PCC Work.**  (a) Bathroom Floor and Rear Verandah Floor over compacted murrum .  (b) Damp Proof Coat (DPC) 2” thick for toilet walls . | Sqft  Sqft | 45  12 |  |  |  |
| 5. | **Foundation Work**.  Shallow strip foundation 2.5ft deep, 1 ft wide wall / strip footing . | Rft | 17 |  |  |  |
| 6. | **Tiling Work**.  (a) Non skid floor tiles in toilet (30sqft)  (b) Wall tiles in toilet upto Dado or 4ft high (70sqft) | Sqft  Sqft | 30  75 |  |  |  |
| 7. | **Toilet Fittings / Plumbing**.  (a)Provision of Indian WC with tap, washbasin (16”) with mirror, tap & shower.  (b) PVC concealed plumbing. | Lumpsum | 01 |  |  |  |
| 8. | **Electrical Work**.  (a) Provision of 1 x ceiling fan hook & point, 04 x LED Light Point,04 x 15/5 Amp Socket at indicated locations.  (b) Electrical wiring in PVC conduits / Casing-Caping fixed to wall. | Lumpsum | 01 |  |  |  |
| 9. | Finishing work to include one coat distemper of ceiling and existing wall | Lumpsum | 01 |  |  |  |
| 10. | Overheads / Additionalities | - |  |  |  |  |
|  | Total |  |  |  |  |  |
|  | GST |  |  |  |  |  |
|  | Grand Total |  |  |  |  |  |

**Note**:- Please attach / Enclose Trade License, GST/TIN, PAN Card details and Earnest Money Instrument.