**BID OF : (***Firm Name***)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**PROJECT: 29 /2020-21 – GARAGE MODIFICATION FOR MAKING KEY STAFF ROOM/QUARTER NO:2 FOR ARMY INSTITUTE OF MANAGEMENT NEW CAMPUS AT RAJARHAT, KOLKATA**

*.Please attach supporting drawings, technical literature / brochure, scanned documents / proof etc as applicable.*

*2. Vendors should be prepared to produce product samples, if applicable.*

*3. The bid preferably be typed on letter head of the firm and authenticated by office stamp & signature on each page.*

*4. Rate quoted should be inclusive of transportation, freight, cartage, handling, fabrication / construction, installation, testing and commissioning at the indicated site, warranty / guarantee liability costs, taxes and levies and any special requirements given in the tender document.*

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S No  | Brief Description / Specifications of Job / Work / Product) or Item(s) | Accounting Unit | Quantity | Rate  | Amount  | Remarks |
| 1. | **Provision of Half Brick Masonry Walls** . Brickwork in CM 1:6.Plaster on both surfaces in CM 1:4.Two coats of dry distemper. | Sqft | 420 |  |  |  |
| 2. | 2. **Provision of Openings : Doors / Windows / Ventilators** .(a) 1 x Single Panel Wooden (Pine) Door (6’ x 2.5’) with frame (Sal) and accessories complete ( inside / outside - locking arrangements– tower &/or sliding bolts, handles, stoppers etc).(b) PVC Door (6’ x 2.5’) with frame and accessories complete ( inside / outside - locking arrangements– tower &/or sliding bolts, handles, stoppers etc).(c)Aluminium Sliding Window (3’ x 2.5’) with security grill, mosquito proofing and accessories complete (handles etc). (d) Ventilator (7’ x 2’) in aluminium frame, 3 equal panels – 2 with fixed glazing & 1 with sliding window. With security grill, mosquito proofing and accessories complete (handles etc).(e) Ventilator (2’ x 1’) in aluminium frame, security grill, mosquito proofing, frosted glass louvere partitions / design. | NosNosNosNosNos | 0102010101 |  |  |  |
| 3. | **RCC Work** . (a) Provision of 9” thick RCC Roof over toiiet with waterproofing treatment.(b) Provision of RCC Lintel over openings. | CuftCuft | 3205 |  |  |  |
| 4. | **PCC Work.**(a) Bathroom Floor and Rear Verandah Floor over compacted murrum .(b) Damp Proof Coat (DPC) 2” thick for toilet walls . | SqftSqft | 4512 |  |  |  |
| 5. | **Foundation Work**.Shallow strip foundation 2.5ft deep, 1 ft wide wall / strip footing . | Rft | 17 |  |  |  |
| 6. | **Tiling Work**.(a) Non skid floor tiles in toilet (30sqft)(b) Wall tiles in toilet upto Dado or 4ft high (70sqft) | SqftSqft | 3075 |  |  |  |
| 7. | **Toilet Fittings / Plumbing**.(a)Provision of Indian WC with tap, washbasin (16”) with mirror, tap & shower.(b) PVC concealed plumbing. | Lumpsum | 01 |  |  |  |
| 8. | **Electrical Work**. (a) Provision of 1 x ceiling fan hook & point, 04 x LED Light Point,04 x 15/5 Amp Socket at indicated locations.(b) Electrical wiring in PVC conduits / Casing-Caping fixed to wall. | Lumpsum | 01 |  |  |  |
| 9. | Finishing work to include one coat distemper of ceiling and existing wall | Lumpsum | 01 |  |  |  |
| 10. | Overheads / Additionalities | - |  |  |  |  |
|  | Total |  |  |  |  |  |
|  | GST |  |  |  |  |  |
|  | Grand Total |  |  |  |  |  |

**Note**:- Please attach / Enclose Trade License, GST/TIN, PAN Card details and Earnest Money Instrument.