|  |
| --- |
|  |

**BID OF : (***Firm Name***)\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**PROJECT : 15 /2020-21 – PROVISION OF PARTITION WALL FOR MEDICAL CENTRE AND JANITOR CLOSETS IN HOSTELS OF ARMY INSTITUTE OF MANAGEMENT NEW CAMPUS AT RAJARHAT, KOLKATA**

*1. Please attach supporting drawings, technical literature / brochure, scanned documents / proof etc as applicable.*

*2. Vendors should be prepared to produce product samples, if applicable.*

*3. The bid preferably be typed on letter head of the firm and authenticated by office stamp & signature on each page.*

*4. Rate quoted should be inclusive of transportation, freight, cartage, handling, fabrication / construction, installation, testing and commissioning at the indicated site, warranty / guarantee liability costs, taxes and levies and any special requirements given in the tender document.*

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| S No | Brief Description / Specifications of Job / Work / Product) or Item(s) | Accounting Unit | Quantity | Rate | Amount | Remarks |
| 1. | **Provision of Partition Wall** .  (a) Installation / Fixing of a full width (7’ x 5’) wooden frame(Sal Wood) with double panel flushed door (Pinewood) complete with standard accessories (door handles, multiple locking arrangements – tower bolts, sliding bolts, stopper etc).  (b) Provision of fixed frosted glazing on aluminium frame and grill above door up to ceiling height to completely block the passage / corridor (5’ x 2’).  (c) Restoration of surfaces as per existing specifications. | Nos  (Lumpsum) | 01 |  |  |  |
| 2. | **Provision of Two Janitor Closets (One Each in Girls & Boys Hostels)**.  (a) Provision of closed L-shaped walk-in janitors closets as per schematic sketch attached.  (b) Cladding and shelves in fibre cement board mounted on aluminium frame.  (c) Provision of access through OVC Door (6’ x 2.5’) on frame with locking arrangements.  (d) Provision of sliding window in aluminium frame with grill (2’ x 2’).  (e) Provision of sloping roof with maximum height 8 ft on one end of the closet, maximum headroom and as per slope profile of stair case.  (d) Provision of wall mounted Kota stone bench (3’ x 1.5’), open shelves (7’ x 3’), mirror (1.5’ x 3’) & six utility hooks as per drawing.  (e) Provision of LED Light Point, 15/5 Amp Socket and Wall Mounted Fan Point.  (e) Restoration work as per existing specifications. | Nos  (Lumpsum) | 02 |  |  |  |
| 3. | Overheads / Additionalities | - |  |  |  |  |
|  | Total |  |  |  |  |  |
|  | GST |  |  |  |  |  |
|  | Grand Total |  |  |  |  |  |